The manuscript is devoted to the problem of acid drainage buffering of copper-nickel sulfide ores enrichment tailings of the Fushë Arrëz flotation plant, Albania. The addition of commercial CaCO3 paste provided by UNICALCE was investigated. The manuscript is well structured. An important positive point is a good combination of geochemical modeling and experimental tests. But there are a number of remarks:
1) In order to understand the scale of the problem, a brief description of old and new tailings: its volume, material composition, content of pyrite and other sulfides.
2) How was FA3 and FA4 sampled? Are these samples averaged?
3) Is it possible to characterize the mineral phases in more detail (Fig. 4.1-4.4) according to X-ray diffraction data, as well as determine its ratio? Reflexes at a number of angles were not identified. Unknown phases?
4) Table 3.1 is replaced by Figure 3.1.

